Input #0, wav, from '.\examples\schedule-hell\schedule-hell.wav':
  Metadata:
    encoder         : FL Studio 2025
  Duration: 00:06:25.21, bitrate: 1411 kb/s
  Chapters:
    Chapter #0:0: start 0.000000, end 19.399002
      Metadata:
        title           : :bpm keyframe 60
    Chapter #0:1: start 19.399002, end 50.366735
      Metadata:
        title           : :bpm keyframe 124
    Chapter #0:2: start 50.366735, end 73.592540
      Metadata:
        title           : drums introduced
    Chapter #0:3: start 73.592540, end 112.302222
      Metadata:
        title           : main synth introduced
    Chapter #0:4: start 112.302222, end 143.269977
      Metadata:
        title           : first break
    Chapter #0:5: start 143.269977, end 158.753832
      Metadata:
        title           : end of first break
    Chapter #0:6: start 158.753832, end 174.237710
      Metadata:
        title           : hi hats introduced
    Chapter #0:7: start 174.237710, end 205.205465
      Metadata:
        title           : second break
    Chapter #0:8: start 205.205465, end 218.753832
      Metadata:
        title           : end first break
    Chapter #0:9: start 218.753832, end 220.689320
      Metadata:
        title           : hiccup start
    Chapter #0:10: start 220.689320, end 251.657075
      Metadata:
        title           : hiccup end
    Chapter #0:11: start 251.657075, end 282.624807
      Metadata:
        title           : third break
    Chapter #0:12: start 282.624807, end 284.560295
      Metadata:
        title           : third break suspension
    Chapter #0:13: start 284.560295, end 331.011905
      Metadata:
        title           : third break end
    Chapter #0:14: start 331.011905, end 361.979637
      Metadata:
        title           : break down start
    Chapter #0:15: start 361.979637, end 377.463515
      Metadata:
        title           : break  down phase 2
    Chapter #0:16: start 377.463515, end 385.205465
      Metadata:
        title           : last bass note
  Stream #0:0: Audio: pcm_s16le ([1][0][0][0] / 0x0001), 44100 Hz, 2 channels, s16, 1411 kb/s
